# No code submission required

# Read the project description (https://fxlin.github.io/p1-kernel/) before proceeding

# Part A: Q&A

This assignment refers to the code under **exp6/**.

1. (5) How many levels of pgtables will we have, if we map memory in sections (2MB)?

There will be three levels of page tables if we map in sections (2MB).

1. (5) What’s the base address of kernel’s virtual address space? What’s the rationale for choosing such a value?

The base address of the kernel’s virtual address space is 0xffff000000000000. The rationale for the base address is that the linker will think that the image is going to be loaded at the base address and will offset as appropriate.

1. (5) What’s the base address of each process’s virtual address space? The rationale for choosing such a value?

The base address is VA\_START

1. (5) When kernel just starts and MMU is off, the CPU should be accessing memory using physical addresses. If that’s the case, how could the kernel possibly access variables (e.g. bss\_start) or functions (e.g. memzero), which are linked at virtual addresses (see pictures below)?

Text

Description automatically generated

(Hint: check the disassembly of the kernel binary that access the variables/functions)

The kernel accesses variables such as **bss\_start** or function such as **memzero** using absolute kernel addresses. In other words, absolute kernel addresses are fixed addresses in physical memory that typically start with *0xffff…*.The linker script specifies the base address of the image and the absolute kernel base addresses are hardcoded in the header where base addresses are defined. Since the absolute kernel addresses typically start with *0xffff…*, this limits access to such variables and functions to only the kernel.

1. (2)

Right after kernel switches to EL1 and clears the BSS, the kernel populates its pgtables via \_\_create\_page\_tables:

// boot.S

\_\_create\_page\_tables:

mov x29, x30 // save return address

The first thing \_\_create\_page\_tables does is to save LR (i.e. x30) to x29. LR points to the address that \_\_create\_page\_tables will return to. Normally, a function would save LR on its stack; this avoids losing the LR value when this function invokes another function with instruction BL, which overwrites LR; when such a function returns, it pops the saved LR value from its stack.

Is it a bug that we save LR to x29?

No, it is not because no code uses the register **x29**. In addition, it saves the return address of the callee. In addition, the **x30** register will get overwritten multiple times by other function calls.

Instead of saving LR to x29, can we save LR by pushing it to stack? Try it out yourself and explain your observation.

In the **\_\_create\_page\_tables** assembly function, I called *stp x30, xzr, [sp, #-8]* which stores the value in the **x30** register to the stack. When running, the kernel simply crashes.

*Changelog*

*Jan 2024. Clarification.*